## Most settings are being done automatically with the sourced variables from setup.env, but you can edit if you need some customization

# Management API

# Management API port
NETBIRD_MGMT_API_PORT=${NETBIRD_MGMT_API_PORT:-33073}
# Management API endpoint address, used by the Dashboard
NETBIRD_MGMT_API_ENDPOINT=https://$NETBIRD_DOMAIN:$NETBIRD_MGMT_API_PORT
# Management Certificate file path. These are generated by the Dashboard container
NETBIRD_LETSENCRYPT_DOMAIN=$NETBIRD_DOMAIN
NETBIRD_MGMT_API_CERT_FILE="/etc/letsencrypt/live/$NETBIRD_LETSENCRYPT_DOMAIN/fullchain.pem"
# Management Certificate key file path.
NETBIRD_MGMT_API_CERT_KEY_FILE="/etc/letsencrypt/live/$NETBIRD_LETSENCRYPT_DOMAIN/privkey.pem"
# By default Management single account mode is enabled and domain set to $NETBIRD_DOMAIN, you may want to set this to your user's email domain
NETBIRD_MGMT_SINGLE_ACCOUNT_MODE_DOMAIN=$NETBIRD_DOMAIN
NETBIRD_MGMT_DNS_DOMAIN=${NETBIRD_MGMT_DNS_DOMAIN:-netbird.selfhosted}
NETBIRD_MGMT_IDP_SIGNKEY_REFRESH=${NETBIRD_MGMT_IDP_SIGNKEY_REFRESH:-false}
NETBIRD_MGMT_DISABLE_DEFAULT_POLICY=${NETBIRD_MGMT_DISABLE_DEFAULT_POLICY:-false}

# Signal
NETBIRD_SIGNAL_PROTOCOL="http"
NETBIRD_SIGNAL_PORT=${NETBIRD_SIGNAL_PORT:-10000}

# Relay
NETBIRD_RELAY_DOMAIN=${NETBIRD_RELAY_DOMAIN:-$NETBIRD_DOMAIN}
NETBIRD_RELAY_PORT=${NETBIRD_RELAY_PORT:-33080}
NETBIRD_RELAY_ENDPOINT=${NETBIRD_RELAY_ENDPOINT:-rel://$NETBIRD_RELAY_DOMAIN:$NETBIRD_RELAY_PORT}
# Relay auth secret
NETBIRD_RELAY_AUTH_SECRET=

# Turn
TURN_DOMAIN=${NETBIRD_TURN_DOMAIN:-$NETBIRD_DOMAIN}

NETBIRD_TURN_EXTERNAL_IP=${NETBIRD_TURN_EXTERNAL_IP}

# Turn credentials
# User
TURN_USER=self
# Password. If empty, the configure.sh will generate one with openssl
TURN_PASSWORD=
# Min port
TURN_MIN_PORT=${TURN_MIN_PORT:-49152}
# Max port
TURN_MAX_PORT=${TURN_MAX_PORT:-65535}

VOLUME_PREFIX="netbird-"
MGMT_VOLUMESUFFIX="mgmt"
SIGNAL_VOLUMESUFFIX="signal"
LETSENCRYPT_VOLUMESUFFIX="letsencrypt"

NETBIRD_AUTH_DEVICE_AUTH_PROVIDER="none"
NETBIRD_AUTH_DEVICE_AUTH_AUDIENCE=${NETBIRD_AUTH_DEVICE_AUTH_AUDIENCE:-$NETBIRD_AUTH_AUDIENCE}
NETBIRD_AUTH_DEVICE_AUTH_SCOPE=${NETBIRD_AUTH_DEVICE_AUTH_SCOPE:-openid}
NETBIRD_AUTH_DEVICE_AUTH_USE_ID_TOKEN=${NETBIRD_AUTH_DEVICE_AUTH_USE_ID_TOKEN:-false}


NETBIRD_DISABLE_ANONYMOUS_METRICS=${NETBIRD_DISABLE_ANONYMOUS_METRICS:-false}
NETBIRD_TOKEN_SOURCE=${NETBIRD_TOKEN_SOURCE:-accessToken}

# PKCE authorization flow
NETBIRD_AUTH_PKCE_REDIRECT_URL_PORTS=${NETBIRD_AUTH_PKCE_REDIRECT_URL_PORTS:-"53000"}
NETBIRD_AUTH_PKCE_USE_ID_TOKEN=${NETBIRD_AUTH_PKCE_USE_ID_TOKEN:-false}
NETBIRD_AUTH_PKCE_DISABLE_PROMPT_LOGIN=${NETBIRD_AUTH_PKCE_DISABLE_PROMPT_LOGIN:-false}
NETBIRD_AUTH_PKCE_LOGIN_FLAG=${NETBIRD_AUTH_PKCE_LOGIN_FLAG:-0}
NETBIRD_AUTH_PKCE_AUDIENCE=$NETBIRD_AUTH_AUDIENCE

# Dashboard

# The default setting is to transmit the audience to the IDP during authorization. However,
# if your IDP does not have this capability, you can turn this off by setting it to false.
NETBIRD_DASH_AUTH_USE_AUDIENCE=${NETBIRD_DASH_AUTH_USE_AUDIENCE:-true}
NETBIRD_DASH_AUTH_AUDIENCE=$NETBIRD_AUTH_AUDIENCE

# Store config
NETBIRD_STORE_CONFIG_ENGINE=${NETBIRD_STORE_CONFIG_ENGINE:-"sqlite"}

# Image tags
NETBIRD_DASHBOARD_TAG=${NETBIRD_DASHBOARD_TAG:-"latest"}
NETBIRD_SIGNAL_TAG=${NETBIRD_SIGNAL_TAG:-"latest"}
NETBIRD_MANAGEMENT_TAG=${NETBIRD_MANAGEMENT_TAG:-"latest"}
COTURN_TAG=${COTURN_TAG:-"latest"}
NETBIRD_RELAY_TAG=${NETBIRD_RELAY_TAG:-"latest"}

# exports
export NETBIRD_DOMAIN
export NETBIRD_TURN_DOMAIN
export NETBIRD_AUTH_CLIENT_ID
export NETBIRD_AUTH_CLIENT_SECRET
export NETBIRD_AUTH_AUDIENCE
export NETBIRD_AUTH_AUTHORITY
export NETBIRD_USE_AUTH0
export NETBIRD_AUTH_SUPPORTED_SCOPES
export NETBIRD_AUTH_JWT_CERTS
export NETBIRD_LETSENCRYPT_EMAIL
export NETBIRD_MGMT_API_PORT
export NETBIRD_MGMT_API_ENDPOINT
export NETBIRD_LETSENCRYPT_DOMAIN
export NETBIRD_MGMT_API_CERT_FILE
export NETBIRD_MGMT_API_CERT_KEY_FILE
export NETBIRD_AUTH_DEVICE_AUTH_PROVIDER
export NETBIRD_AUTH_DEVICE_AUTH_CLIENT_ID
export NETBIRD_AUTH_OIDC_CONFIGURATION_ENDPOINT
export NETBIRD_AUTH_REDIRECT_URI
export NETBIRD_AUTH_SILENT_REDIRECT_URI
export TURN_DOMAIN
export TURN_USER
export TURN_PASSWORD
export TURN_MIN_PORT
export TURN_MAX_PORT
export VOLUME_PREFIX
export MGMT_VOLUMESUFFIX
export SIGNAL_VOLUMESUFFIX
export LETSENCRYPT_VOLUMESUFFIX
export NETBIRD_DISABLE_ANONYMOUS_METRICS
export NETBIRD_MGMT_SINGLE_ACCOUNT_MODE_DOMAIN
export NETBIRD_MGMT_DNS_DOMAIN
export NETBIRD_MGMT_IDP_SIGNKEY_REFRESH
export NETBIRD_SIGNAL_PROTOCOL
export NETBIRD_SIGNAL_PORT
export NETBIRD_AUTH_USER_ID_CLAIM
export NETBIRD_AUTH_DEVICE_AUTH_AUDIENCE
export NETBIRD_TOKEN_SOURCE
export NETBIRD_AUTH_DEVICE_AUTH_SCOPE
export NETBIRD_AUTH_DEVICE_AUTH_USE_ID_TOKEN
export NETBIRD_AUTH_PKCE_AUTHORIZATION_ENDPOINT
export NETBIRD_AUTH_PKCE_USE_ID_TOKEN
export NETBIRD_AUTH_PKCE_DISABLE_PROMPT_LOGIN
export NETBIRD_AUTH_PKCE_LOGIN_FLAG
export NETBIRD_AUTH_PKCE_AUDIENCE
export NETBIRD_DASH_AUTH_USE_AUDIENCE
export NETBIRD_DASH_AUTH_AUDIENCE
export NETBIRD_STORE_CONFIG_ENGINE
export NETBIRD_DASHBOARD_TAG
export NETBIRD_SIGNAL_TAG
export NETBIRD_MANAGEMENT_TAG
export COTURN_TAG
export NETBIRD_TURN_EXTERNAL_IP
export NETBIRD_RELAY_DOMAIN
export NETBIRD_RELAY_PORT
export NETBIRD_RELAY_ENDPOINT
export NETBIRD_RELAY_AUTH_SECRET
export NETBIRD_RELAY_TAG
export NETBIRD_MGMT_DISABLE_DEFAULT_POLICY
